Chain Assembly Inspection 
Inspection of the chain assembly is an integral part of the daily inspection of the PODZILLA Lift System.  The chain assembly should always be inspected for rust, inadequate lubrication, excessive dirt or misalignment of the chain assembly with the sprocket assembly. Also verify all teeth are located throughout the entire sprocket assembly to ensure safe and continued operation throughout the scheduled day’s route.
 
	Step 1          Identify right drive wheel chain assembly.
Step 2          Inspect the chain assembly for rust, excessive dirt and alignment.
Step 3          Check the chain for slack.  Rotate wheel so chain slack is on top of the sprockets.  Lay a straight edge on top of the chain rollers.  Measure the distance between the chain and the straight edge.  This distance should never be less than ¾”.
Step 4          Inspect the sprocket assembly for missing teeth.
Step 5          Spray chain lube onto chain assembly as necessary.
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