Hydraulic Fluid Verification
Verify the hydraulic fluid level is accurate as the PODZILLA lift is on/off the bed of the PODS delivery truck.  Inspect the gauge to verify there are no cracks or leaks which would ​​hinder the ability to obtain and accurate reading. 
 
		Step 1           Inspect the Sight Gauge for cracks or leaks.
Step 2           Verify hydraulic fluid fill minimum of 1/3 on Sight Gauge if the PODZILLA lift is ON the truck.
Step 3           Verify hydraulic fluid fill maximum of 2/3 on Sight Gauge if the PODZILLA lift is OFF of the truck.
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