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Friction causes heat and heat can be very destructive to mechanical and electrical components. Lubrication acts to reduce the friction of moving parts, thereby lowering operating temperatures. Like most mechanical equipment, the PODZILLA Lift System requires adequate lubrication to operate at maximum efficiency over a prolonged time.
 
	Skills Required:  
	Low/Moderate

	Tools Required:       
	Monolith AW2 (or equivalent) lubricating grease

	 
	Old leather/rubber glove or paint brush

	 
	Grease gun (for zerk fittings)


 
Lubricate the four lift legs and two spreader bars with grease. Extend all four lift legs and open the spreader bars. Use Monolith AW2 lubricating grease (or equivalent) and apply smooth, even coating using an old glove or paintbrush. Leave about 2’ of lift leg dry and free from grease.
 
· Lube the zerk fittings on the four front drive wheels. Using the grease gun, fill the zerk fitting with grease until there is an overflow escape from the fitting  .
· Lube zerk fittings on two guide wheels. Using the grease gun, fill the zerk fitting with grease until there is an overflow escape from the fitting.
· Lube zerk fittings on caster wheel assemblies. Using the grease gun fill the zerk fitting with grease until there is an overflow escape from the fitting.
 
 

