Main Beam Seam Weld
Left and Right Side
It is imperative to inspect all 9 main beam seam welds along the top and bottom of the main beam.  Physically look under the main beam assembly to verify no cracks, breaks or separations are apparent in any of the welds throughout the main beam assembly.
 
	Step 1              Identify Main Beam Seam Weld.
Step 2              Inspect the main beam assembly for cracks, breaks or separations.
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