Tires - Caster and Drive

Inspect and verify the correct tire pressure in each tire to ensure safe and efficient operation.  Unstable movement and blown out tires are a direct reflection of low air pressure.  In order to achieve maximum maneuverability and the ability to climb inclines the air pressure should be in accordance with the     recommended tire pressure indicated on the tire.
 
Inadequate tire pressure and poor tire condition will cause performance issues and failures. In addition, tire condition affects the longevity of bearings and axles. Cracking of the axle will leave a lift grounded and is a direct result of uneven air pressure in tires. Finally, the customer's experience is diminished if tire marks are left on the driveway, and this is usually caused by tires being under-inflated or unevenly mated.
 
	Step 1              Identify Front Caster Tires and Rear Drive Tires

Step 2              Inspect the tires for excessive wear, cracks or punctures.

Step 3              Verify listed load range and tire pressure on sidewall of tires.

Step 4              Verify lug nuts are secure and snug. 
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