Wear Disk Cap Plate Bolts 

Inspect and verify all 32 wear disk cap plate bolts are tight and secure.  Loose operation of the PODZILLA Lift System will occur if these bolts are not secure.  Failure to tighten these bolts will result uneven wear of the ram assemblies which can lead to equipment failure and unnecessary down time.  Use a 9/16” wrench to tighten all bolts to ensure safe and efficient lift operation.
 
	Step 1  Identify Wear Disk Cap Plate Bolts
Step 2  Verify the wear disk cap plate bolts are located in the plates.
Step 3  Verify the wear disk cap plate bolts are secure. 
 

	Alternate (Simple) Inspection:
Grab the bottom of the wheel leg while leg is in the up position and shake it back and forth. The leg should have a bit of play in it.  When the play is between 1/3” and 1/2”, visually inspect and, if necessary, replace the bolts or warn Wear Disc.​



