


Lift Chain Assembly Inspection

Verify the lift chain assembly is secure and has NO signs of weakness in the chain links.  It is imperative to inspect the cotter pins on the lift chain assembly to ensure safe and efficient lift operation.
 
	Step 1           Identify Lift Chain Assembly
Step 2           Verify complete chain assembly with chain chokers.
Step 3           Inspect chain assembly for cracks or elongated links.
Step 4           Look for mushroomed wear at last link to slider.
Step 5           Verify cotter pin installed.
Step 6           Inspect cotter pin for damage.
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