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	Podzilla Annual Certification Checklist

	☐	Inspect engine for proper service  (3 points)

	☐	Inspect for air filter change  (2 points)

	☐	Inspect for proper water level in battery  (2 points)

	☐	Inspect all wheel lugs  (3 points)

	☐	Inspect wear disk cap plate bolts and hardware  (3 points)

	☐	Inspect fuel filter for proper replacement  (3 points)

	☐	Inspect hydraulic filter for proper replacement  (3 points)

	☐	Inspect all driver and caster bearings for proper lubrication  (3 points)

	☐	Inspect all inner steel tubes for proper lubrication  (3 points)

	☐	Inspect and check all frame and weld joints for damage or cracks  (3 points)

	☐	Inspect chain eyelets for excessive wear  (3 points)

	☐	Inspect chain assemblies for correct cotter-pin placement  (3 points)

	☐	Inspect tires for excessive rim and tire damage  (3 points)

	☐	Check tires for recommended PSI  (3 points)

	☐	Inspect all drive and castor assemblies for signs of leaks  (3 points)

	☐	Inspect hydraulic fluid for proper levels and contamination  (3 points)

	☐	inspect hydraulic pump assembly  (3 points)

	☐	Inspect ignition assembly  (3 points)

	☐	Perform engine run test  (3 points)

	☐	Perform hydraulic pressure test  (3 points)

	☐	Inspect wear disc cap  plates and hardware  (3 points)

	☐	Inspect and calibrate all remote systems (remote models only)  (3 points)

	☐	Inspect all valve systems for damage and leaks  (3 points)

	☐	Inspect spreader wheel assemblies  (3 points)

	☐	Inspect all cascade reels and hoses for damage and leaks  (3 points)

	☐	Inspect castor assembly lockout position  (3 points)

	☐	Inspect for pressure wash and degreasing [wash as needed]  (3 points)

	☐	Inspect paint for adherence to brand standards [paint as required]  (3 points)

	☐	Inspect signage and brackets  (3 points)

	☐	Inspect all decals  (3 points)

	☐	Inspect drive valve for correct tracking  (3 points)

	☐	Inspect all hoses and fittings  (3 points)

	☐	inspect guide wheel assembly  (3 points)

	☐	Inspect all hose block assemblies  (3 points)
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