Ram Assembly


	Inspection of the ram assembly is imperative to the operation of the PODZILLA lift system. Inspect all weld points throughout the entire perimeter of the ram assembly to en​​​​sure safe and efficient lift operation. Verify all 4 welds along the ram assembly are inspected for any cracks, breaks or separations. 

	​
Step 1 Identify right rear ram assembly 
Step 2 Inspect the welds along all edges of the Ram Assembly for cracks, breaks or separations. 
Step 3 Scan the designated barcode.

	​[image: A warning sign on a metal post

Description automatically generated]



image1.jpeg
18 12:54pH





