           RG Podzilla Transport Acceptance Check List

· Review Transport’s BOL/Manifest to ensure Podzilla is being delivered to the correct location and the Podzilla Serial number matches the transport paperwork.
· Verify that the Remote Belly Box, (2) Remote Batteries, Battery Charger, and Tether Cord are accounted for and should be listed on the transport paperwork. 
· Take pictures of the Podzilla immediately upon transport arrival and before Podzilla is unloaded from the PODS Truck or Low Load Trailer.  Pictures should include:
a. Overview picture showing the entire Podzilla from both ends and each side.
b. Pictures of any damage or missing parts.
c. Picture of the Patent Plate.
· Perform a Podzilla DVIR and report defects to cvillemaire@pods.com for warranty submittal.
· Fill out the Fixed Asset’s Equipment Add Form and send it to fixedassetsaccounting@pods.com
· Complete a full Podzilla PM prior to placing Podzilla into service.
· Operate the Podzilla manually and with the remote control using both Rabbit Mode and Turtle Mode to confirm proper operation of the Remote System prior to placing the Podzilla into service.

